###### RK INTERNATIONAL MACHINE TOOLS LTD

**Europa Trading Estate, Fraser Road, Erith, Kent DA8 1PW. England**

**Tel. No. 01322 447611 Facsimile No. 01322 447618**

**E-mail:** sales@rk-int.com **Website:** [www.rk-int.com](http://www.rk-int.com/)

**Used Haas Model VF3 Vertical CNC Machining Centre**

**Serial Number: 1081462**

**Year of Manufacture: 2011**

|  |  |
| --- | --- |
| **Specification** |  |
| **Travel** |  |
| X axis stroke | 1016mm |
| Y axis stroke | 508mm |
| Z axis stroke | 635mm |
| Distance spindle nose to table | 102-737mm |
| **Table** |  |
| Width | 457mm |
| Length | 1219mm |
| Max. Weight on table | 1588kg |
| T Slots : width | 16mm |
|  : pitch | 80mm |
| **Spindle** |  |
| Taper size | No.40 |
| Speed | 0-10,000rpm |
| **Bearings** |  |
| Bearing lubrication | Air/oil injection |
| Cooling | Liquid cooled |
| **Motor** |  |
| Spindle motor, max. rating | 14.9kW |
| **Feedrate** |  |
| Rapid X, Y & Z axis  | 25.4m/min |
| Max. Cutting feedrate | 16.5m/min |
| **Toolchanger** |  |
| Capacity | 20 tools |
| Type | BT40 |
| **General** |  |
| Approximate machine weight | 5670kg |
| Air supply (min) | 113lpm, 6.9 bar |

|  |
| --- |
| **Machine equipped with:-** |
| Haas (Fanuc compatible) CNC Control system |
| Through spindle coolant |
| Wireless intuitive probing system |
| High speed machining |
| Programmable coolant nozzle |
| Automatic lubrication system |
| Enclosed guarding |
| Swarf auger |
| Lighting |