|  |  |
| --- | --- |
| **SPECIFICATION** |  |
| Trunnion table size | 630mm x 500mm |
| X axis traverse | 762mm |
| Y axis traverse | 508mm |
| Z axis traverse | 508mm |
| B axis tilt | +110 deg -35 deg |
| C axis rotation | 360 degree |
| Spindle | BT 40 |
| Spindle speeds | 0-15,000rpm |
| Spindle motor | 22.4kW |
| Rapid feed rate X,Y,Z axis | 30.5m/min |
| Rapid feed rate B,C axis | 150 degrees a second |
| Toolchanger capacity | 40 + 1 tools |
| Approx. weight | 8900kg |

|  |
| --- |
| **MACHINE EQUIPPED WITH:-** |
| Haas CNC control system |
| Through spindle coolant, with auxiliary filtration |
| Swarf conveyor |
| Wireless Intuitive Probing System |
| Lighting |
| Enclosed guarding |