**Used Colchester Combi 3000**

 **Electronic Centre Lathe**

**Serial Number: E40018**

**Year Of Manufacture 1998**

|  |  |
| --- | --- |
| **Specification**  |  |
| Swing over bed | 460mm |
| Swing in gap | 730mm |
| Swing over cross slide | 270mm |
| Distance between centres | 2000mm |
| X axis cross slide travel | 300mm |
| Spindle nose (Camlock) | D1-8 |
| Spindle bore | 76mm |
| Spindle motor | 18.5/22kW |
| Spindle speeds (programmable) | 20-2000rpm |
| X axis ballscrew, diameter x pitch | 25 x 4mm |
| Z axis ballscrew, diameter x pitch | 40 x 10mm |
| Tailstock quill taper | No. 6 MT |
| Tailstock quill travel | 145mm |
| Bedway width | 400mm |
| Approximate nett weight | 3750kg |

|  |
| --- |
| **Machine Equipped with** |
| Fanuc 210i TA CNC Control |
| 3 Jaw chuck |
| Parat toolpost and 2 off toolholders |
| Guarding |
| Coolant system |
| Lighting |

**Price £**