**Used Quaser MF500-C 4 plus 1 axis Vertical Machining Centre**

**Serial Number: 307B100029**

**Year of Manufacture: 2009**

|  |  |
| --- | --- |
| **Specification** |  |
| X Axis travel | 550mm |
| Y Axis travel | 630mm |
| Z Axis travel | 610mm |
| A Axis travel (degree) | +30° ~-120° |
| C Axis travel (degree) | 360° (Continuous) |
| Table diameter | 410mm |
| Maximum swing diameter | 500mm |
| Maximum workpiece size | 500mm dia x 300mm high |
| Table load capacity | 200Kg |
| Spindle taper | BBT40 face and taper |
| Spindle rpm | 12,000rpm |
| Spindle power | 17.6kW (S6-25%) |
| Spindle torque | 112Nm (S6-25%) |
| Automatic tool changer | 60 station |

|  |
| --- |
| **Machine equipped with:-** |
| 20 bar through spindle coolant |
| Renishaw NC4 and OMP60 probes |
| Swarf conveyor |
| Filtermist extraction |
| Visi-Port window |
| 20 bar through spindle coolant |

**Price £**

**NB** Machine ex works Bristol