**Used Colchester Triumph VS 2500 Gap Bed Centre Lathe**

**Serial Number: LVT25GMRJA/05404**

**Year of Manufacture: 1991**

|  |  |
| --- | --- |
| **Machine specification** |  |
| Height of centres | 195mm |
| Swing over bed | 400mm |
| Swing over cross slide | 246mm |
| Swing in gap | 585mm |
| Width in front of faceplate | 165mm |
| Bed length between centres | 650mm |
| Spindle speeds (infinitely variable) | 0-2500rpm |
| Spindle nose mounting | (Camlock) D1-6 |
| Spindle bore | 54mm |
| Spindle motor | 7.5kW |
| Width over bedways | 318mm |
| Travel of cross slide | 250mm |
| Travel of top slide | 130mm |
| Travel of tailstock barrel | 178mm |
| Taper in tailstock barrel | No. 5 MT |
| Approx. Weight | 1400kg |
| Machine in **Metric** execution | |

|  |
| --- |
| **Machine equipped with** |
| Heidenhain 2 axis DRO system |
| 3 Jaw chuck |
| Ainjest high speed screwcutting attachment |
| Taper turning attachment |
| Quick change toolpost and 3 off toolholders |
| Lighting |
| Coolant System |
| Rear splashguard |