|  |  |
| --- | --- |
| **SPECIFICATION** |  |
| Grinding Length between Centres | 305mm |
| Maximum swing | 125mm |
| Table swivel angle | +/-10º |
| Range of Work head Speeds (inf. Variable) | 100 – 900rpm |
| Standard Grinding Wheel | 305 x 38 x 127mm |
| Wheel head Speeds (2) | 1830 /1988rpm |
| Wheel head motor | 2.2Kw |
| Cross Traverse of Wheel head | 98mm |
| Approx. Weight | 900kg |
| Machine in Metric execution |  |

|  |
| --- |
| **Machine equipped with** |
| Swing down internal grinding attachment |
| Assorted collets |
| Coolant system |
| Guarding |