Hembrug Mill-Turn Machine 
Model: Slantbed Mikroturn 100 CNC
Siemens 840D Control
Approximate Actual Run Time Hours: 1,000 
Hydrostatic Spindle
Hydrostatic Ways
Scale Feedback
Suspended Granite Bed
Granite Spindle Housing
Coolant Pump
Coolant Circulation Pump
Pneumatic Bearing Purge
Hydraulic Temperature Control
Coolant Temperature Control
Return Oil Pump and Reservoir for Remote Location of Hydraulic / Cooling Unit.


Options & Additional Purchased Features:
Tailstock
Vacuum Pump for Vacuum Chucking
Programable Controlled Spray Mist 
C-Axis Milling / Drilling
Renishaw Tool Touch Probe
Non-Contact Tool 
Incoming Air Dryer / Filter

Thousands of Dollars of Brand New Tooling:
Live Center
Tailstock Taper Adapter
8” Micro-Centric Pneumatic Chuck
3 Sauter Straight Live tooling heads 
2 Sauter 90 degree Live tooling heads
1 Special VDI offset Tooling holder
16 VDI Tool Holders for Turning, boring, and on center drilling.
Tool Pick-up Video System
Additional Backup Hard Drive with Software Fully Loaded and Tested. 
Extra Siemens Control Pannel
Complete Set of Manuals

Machine Upgrades I added at additional cost.
New Digital Hard Drive
New Backup Hard Drive with software already loaded, plug and play ready, no downtime.
New Z-Axis Heidenhain Scale
Rewound Hydraulic Pump Motor, factory motor was running too hot for my liking.
Replaced Operator Panel, back light on monitor went out, have the original, back light needs replacing. 
50  Foot Extended Wiring Harness For Remote Location of Hydraulic / Cooling Unit.

