###### RK INTERNATIONAL MACHINE TOOLS LTD

**Europa Trading Estate, Fraser Road, Erith, Kent DA8 1PW. England**

**Tel. No. 01322 447611 Facsimile No. 01322 447618**

**E-mail:** [sales@rk-int.com](mailto:sales@rk-int.com) **Website:** [www.rk-int.com](http://www.rk-int.com/)

**Used XYZ 750LR Vertical Machining Centre**

**Serial Number: SMA10217**

**Year of Manufacture: 2021**

|  |  |
| --- | --- |
| **Specification** |  |
| X Travel | 750mm |
| Y Travel | 440mm |
| Z Travel | 500mm |
| Table size | 830 x 410mm |
| Spindle centre to column | 500mm |
| Spindle to table | 100 – 600mm |
| Colum front to table centre | 305 – 745mm |
| Rapid feed XYZ axis | 20M/min |
| Cutting feedrates | 1-20,000mm/min |
| Max table load | 500kg |
| T slot size | 16mm |
| T slot number and pitch | 3 @ 100mm |
| Spindle speed | 5 – 8000rpm |
| Spindle motor | 15Kw |
| Spindle taper | BT40 |
| Tool magazine capacity | 20 |
| Max tool diameter | 80mm |
| Max tool weight | 7kg |
| Coolant capacity | 125L |
| Ball screw size (grade C3) | 32mm P8 |
| Machine weight | 3500kg |
| Footprint W x D X H | 2100 x 2150 x 2450mm |

|  |
| --- |
| **Machine equipped with:-** |
| Siemens 828D CNC Control |
| Swarf conveyor |
| Enclosed guarding |
| Lighting |
| Coolant system |