###### RK INTERNATIONAL MACHINE TOOLS LTD

**Europa Trading Estate, Fraser Road, Erith, Kent DA8 1PW. England**

**Tel. No. 01322 447611 Facsimile No. 01322 447618**

**E-mail:** **sales@rk-int.com** **Website:** [**www.rk-int.com**](http://www.rk-int.com/)

**Used Europa VS660 Gap Bed Centre Lathe**

**Serial Number: 0153**

**Year of Manufacture: 2013**

|  |  |
| --- | --- |
| **Specification** |  |
| Centre height | 330mm |
| Distance between centres | 1500mm |
| Swing over bed | 660mm |
| Swing over cross slide | 430mm |
| Spindle bore (max. bar dia) | 104mm |
| Spindle nose mounting | D1-11 Camlock |
| Taper in spindle bore | No. 7 Morse |
| Swing in gap | 860mm |
| Width of bedways | 480mm |
| Total travel of cross slide | 390mm |
| Total travel of top slide | 190mm |
| Total travel of tailstock barrel | 300mm |
| Spindle speeds (infinitely variable) | 18 – 1400rpm |
| Drive vee belt and clutches |  |
| Spindle motor | 20HP |
| Imperial pitches (73) | 2-84TPI |
| Diametral pitches (27) | 8-72DP |
| Metric pitches (51) | 0.2 – 14mm |
| Module pitches (20) | 0.2 –3.5 MOD |
| Approx. weight | 3800 kg |
| Machine in Imperial execution |  |

|  |
| --- |
| **Machine equipped with** |
| Fagor 2 axis DRO system |
| 3 jaw chuck |
| Quick change toolpost and toolholders |
| Rapid power traverse to saddle |
| lighting |
| Coolant system |
| Chuck guard |
| Rear splash guard |

**Price £37,500.00**